Salient Characteristics
400-Ton Chiller 
Basis of design: YORK model YCAV0457PA46VACBXT
Power requirements: 480VAC 3-phase 60Hz maximum load of 781A
Refrigerant type: R-134A
100-Ton Chiller
Basis of design: YORK model YLAA0100ZE46XBABXT
Power requirements: 480VAC 3-phase 60 Hz maximum load 223A
Refrigerant type: 410A

