

	NSN:   LLS053476                                                                             

HOSE, AIR DUCT

6" ID X 25' LONG

NEOPRENE/POLYESTER 2 PLY WITH SPRING STEEL WIRE, FLEXIBLE
COLOR - BLACK 

MUST BE PALLETIZED. DUCTING TO BE PAINT STENCILED OR INK PRINTED: "FIRE RESISTANT      PROPERTY OF US NAVY"
                                      or
                  FIRE RESISTANT     
                  PROPERTY OF US NAVY


ON THE DUCT  in 1-1/8" -  1- ½ " TALL WHITE CHARACTERS IN AT LEAST EIGHT LOCATIONS, DISTRIBUTED ALONG THE LENGTH AND ALL SIDES OF THE DUCT.  If the text is on one line, there shall be 8 to 12 inches spacing between the words  "RESISTANT" and "PROPERTY".


Known compliant ducts:  

Flexaust - CWGP 
[bookmark: _GoBack]Hi-Tech Duravent - 2PN
