

	NSN:   LLS039956                                                                          

HOSE, AIR DUCT

8-1/2" ID X 25' LENGTH.  1.25" PITCH HELICAL WOUND WIRE.  NEOPRENE, 2 PLY, UL-94-V-0, 12 GAUGE WIRE, FOR FUNE/AIR DUST.

MUST BE PALLETIZED. DUCTING TO BE PAINT STENCILED OR INK PRINTED: "FIRE RESISTANT      PROPERTY OF US NAVY"
                                      or
                  FIRE RESISTANT     
                  PROPERTY OF US NAVY


ON THE DUCT  in 1-1/8" -  1- ½ " TALL WHITE CHARACTERS IN AT LEAST EIGHT LOCATIONS, DISTRIBUTED ALONG THE LENGTH AND ALL SIDES OF THE DUCT.  If the text is on one line, there shall be 8 to 12 inches spacing between the words  "RESISTANT" and "PROPERTY".


Known compliant ducts:  

Flexaust - CWGP
Flexaust - CWC 18-1/2" x 25'  
[bookmark: _GoBack]Hi-Tech Duravent - 2PN
