Battery Specs for Permanent Count Sites

LiFePo4 Battery 12V 52Ah Group 31 case
Dimensions- No larger than 8”x 7”x 7”
Waterproof Rating IP67
High impact case
Flame retardant case
Fully automatic low temperature charging with integrated heater
Battery charge temps ( -4 to 113 Degree or higher)
Cycle life – 3000+
[bookmark: _Hlk205450072]Built in Battery Management System (BMS)

LiFePo4 Battery 12V 100Ah Group 31 case
Dimensions- No larger than 13”x7”x 9” 
Waterproof Rating IP67
High impact case
Flame retardant case
Fully automatic low temperature charging with integrated heater
Battery charge temps ( -4 to 113 Degree or higher)
Cycle life – 3000+ 
Built in Battery Management System (BMS)

LiFePo4 Battery 12V 300Ah Group 31 case 
Dimensions- No larger than 21”x11”x 9” 
Waterproof Rating IP67
High impact case
Flame retardant case
Fully automatic low temperature charging with integrated heater
Battery charge temps ( -4 to 113 Degree or higher)
Cycle life – 3000+ 
Built in Battery Management System (BMS)

