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INTRODUCITON:
The Defense Logistics Agency-Aberdeen, on behalf of the Army Integrated Logistics Supply Center (ILSC), intends to acquire Parts to support the Electric Power Plant (EPP) III.  The EPP III is the main electric power source for the PATRIOT Missile Defense System, and the selected parts have been identified for maintenance and sustainment purposes.   The parts consists of various cables, conduits, and a reel on which cabling sits. These cables are used between the Power Distribution Unit to the Generator Sets.

APPLICABLE DOCUMENTS
	Military and Federal Standards
	

	MIL-STD-130N w/Change 1
	Identification Marking of U.S. Military Property

	MIL-STD-129R w/Change 3
	Military Marking for Shipment and Storage

	MIL-STD-2073-1E w/ Change 4
	Standard Practice for Military Packaging

	Military and Federal Specifications
	

	N/A
	

	Other Documents
	

	Commercial Documents
	

	ISPM Number 15
	Regulation of Wood Packaging Material in International Trade

	ANSI/TA-STD-0016
	Standard for Preparing a Diminishing Manufacturing Sources and Material Shortages (DMSMS) Management Plan

	ANSI/ISO/ASQ(E)Q 9001-2015
	American National Standard, Quality Management Systems-Requirements

	Security Documents
	

	CECOM G2

	Antiterrorism/OPSEC /Security Cybersecurity Review Cover Sheet



[bookmark: _Toc119572189]CONFIGURATION BASELINE
The applicable Configuration Baselines (CB), for the listed Configuration Item (CI) and/or Computer Software Configuration Item (CSCI), are as listed in the table below.

	NSN
	Nomenclature
	Part Number

	6150-12-343-3731
	CABLE ASSEMBLY,SPEC
	180.01.0501

	6150-12-343-3732
	CABLE ASSEMBLY,SPEC
	180.01.0504

	6150-12-343-3733
	CABLE ASSEMBLY,SPEC
	180.01.0058

	6150-12-343-3734
	CABLE ASSEMBLY,SPEC
	180.01.0502

	6150-12-343-3735
	CABLE ASSEMBLY,SPEC
	180.01.0503

	6150-12-343-3736
	CABLE ASSEMBLY,SPEC
	180.01.0050

	6150-12-343-3737
	CABLE ASSEMBLY,SPEC
	180.01.0505

	6150-12-343-3738
	CABLE ASSEMBLY,SPEC
	180.01.0148

	6150-12-343-3739
	CABLE ASSEMBLY,SPEC
	180.01.0149

	5975-12-343-4086
	CONDUIT ASSEMBLY
	115.02.0016

	5975-12-343-4089
	CONDUIT ASSEMBLY
	115.02.0010

	8130-12-358-4625
	REEL CABLE
	480.02.0047

	5945-01-577-2614
	RELAY, HYBRID
	335.01.0040

	5975-12-343-4088
	CONDUIT ASSEMBLY
	115.02.0006
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[bookmark: _Toc119572191]Part Revisions 

Departures from Configuration Baseline (CB).  No changes or departures from the CB are acceptable except for changes or departures which are submitted in accordance with DI-MISC-80711A and are approved by the Government Configuration Manager (C Mgr.) or Configuration Management Officer (CMO) and which are made applicable to the contract by the PCO.  Configuration Control shall be affected by the Configuration Control Documents (CCDs) as follows:

Engineering Change Proposal (ECP) includes both the engineering change and the supporting documentation by which the change is described and suggested.  An ECP describes changes to the CI/CSCI and associated Government documents and data that are affected by the proposed engineering change.

A Notice of Revision (NOR) shows the detailed changes that must be made to technical documentation, except specifications, (one NOR per document) following approval of an ECP.  The NOR is submitted as part of the ECP and is used to determine any Technical Manual (TM) impacts. The Government must be notified of any part changes in order to update the proper TMs. 

A Specification Change Notice (SCN) is used to delineate the exact change(s) in a specification that will be distributed to users when the ECP is approved.  The SCN is submitted as part of the ECP.  The SCN is not used for a military or federal document, only a Request for Waiver can be used for those documents.

Value Engineering Change Proposal (VECP) is the same as an ECP except there are proposed cost savings for the program.  The contractor shall follow the guidance in Section I of this contract for VECPs. 

Request for Waiver (RFW) describes a departure from configuration documentation for a specific number of units or period of time.  Contractor shall identify the impact of the RFW on performance, operational readiness and logistics support of the affected CIs.  The Government will require compensation for any RFW.

Contractor shall provide all supporting program or cost data with the CCD.  The contractor shall uniquely and sequentially identify (including the use of the contract number) each ECP, VECP, NOR, SCN or RFW.  The identification number should use less than 16 characters.

Identification of Authorized Personnel.  The contractor shall identify to the PCO, Administrative Contracting Officer (ACO), and the technical office identified on the DD Form 1423 for DI-MISC-80711A, the name(s) of the official(s) of its organization who are authorized to submit CCDs 30 Days after Contract (DAC).

Documentation.  The contractor shall document by serial number each products configuration, applicable documentation, maintenance support requirements and spares in relation to the contractor’s configuration baseline.  The data in use shall be available for government review and use.

Use of CB Data.  The contractor shall assure that all necessary contractor’s activities have access to and use of the contractually specified configuration baseline(s), approved changes and departures, and effectivity data.  The data in use shall be available for government review and use.
[bookmark: _Toc119572192]SPECIAL INSTRUCTIONS

Requirements for Item Marking (Commercial Off The Shelf Items).  Part Number Marking.  Each item delivered under contract, along with each assembly, sub assembly, and module, shall be legibly marked with the appropriate part number and manufacturer’s identification. Hardware such as screws, nuts, bolts, etc., need not be marked.  This requirement should be entirely met by the contractor’s standard commercial marking. However, if there is any question about marking it shall be directed to the Contracting Officer for resolution.

Requirements for Item Unique Identification (IUID).  The contractor shall mark all contract deliverables In Accordance With (IAW) DFARS clause 252.211-7003 in this contract and the following requirements.  

IUID Marking.  

IUID markings shall be IAW MIL-STD-130N. 

Commercial Markings.

Permanency and Legibility.  The IUID marking and identification plates, tags, etching, or labels when used on equipment, parts, assemblies, subassemblies, units, sets, groups, or kits shall be as permanent as the normal life expectancy of the item and be capable of withstanding the environment, test, cleaning, repair, and rebuild procedures specified for the item.  Legibility shall be as required and verified for ready readability per MIL-STD-130N.  

Deleterious Effect.  Marking of items shall be accomplished in a manner that will not adversely affect the life and utility of the item. Marking materials creating hazardous conditions shall not be used. Placement and choice of the marking shall not create hazardous conditions.

IUID Coding.  IUID markings and readability requirements shall comply with MIL-STD-130N.

Symbology markings and the order of priority for marking the hardware shall be in accordance with MIL-STD 130N.  First priority is the 2D data matrix symbol (machine readable) IUID is the minimum requirement when there are severe space limitations. The second priority is the human readable characters. The third priority is the Linear Bar Code.   
If the technical data has not specified the marking location, markings shall be located such that they are visible during item use, provided that sufficient space is available, and does not interfere with equipment operations. 

If items are not described by Government Product Technical Data (i.e. Commercial Items), the contractor shall submit diagrams showing placement and description of the IUID marking and applicable installation and processing instructions for government review and approval IAW with CDRL for DI-MISC-80711A and this Technical Requirements Document (TRD).

The contractor shall maintain an accurate, current list of IUIDs for all manufactured items on this contract.  Dates of manufacture, substitutions, shop changes, etc. shall be included on this list.  The list shall be available for inspection by the PCO or other Government representative at any time during the life of this contract.  The contractor shall provide this list to the government at the end of the contract.

Pricing of IUID Requirements.  All efforts required by this TRD and contract, including, but not limited to, the preparation of ECPs or notification of marking deficiencies, PIPC reporting, serial number data reporting at end of contract and the actual marking of hardware, will be included in the base unit price.

[bookmark: engr10end]Requirements for Final Inspection and Test . The contractor shall implement and maintain a Final Inspection and Test System that meets or exceeds the requirements established below. These requirements are commonly accepted practices employed by industry. 

Quality System . The contractor shall establish/maintain an effective inspection and test system for final inspection and test of completed products IAW ANSI/ISO/ASQ(E) Q9001-2015. 

Inspection and Testing Procedures . The contractor shall utilize documented procedures for final inspection and testing of finished products to ensure that all contract requirements are satisfied. 

Inspection and Testing . The quality system shall assure that all final inspections and tests required satisfying contract requirements are conducted. 

Records . The contractor shall maintain adequate records of final inspections and tests to demonstrate that the product satisfies contract requirements. 

Measuring, Testing, and Inspection Equipment . The contractor shall provide and maintain gages (including production tooling used for inspection purposes) and other measuring and testing equipment to assure that finished products conform to contract requirements. These devices shall be calibrated against certified measurement standards that are traceable back to national/international standards. 

Inspection and Test Status . The contractor shall maintain a system for the identification of the final inspection and test status of all products. 

Nonconforming Material . The contractor shall establish and maintain a system for controlling material that does not satisfy contract requirements, including procedures for its identification, segregation, and disposition (rework/repair, scrap, etc.). 

Corrective Action . The contractor shall promptly act to correct nonconforming materials and processes to preclude the recurrence of the problem and to satisfy contract requirements. 

Training Requirements . The contractor shall identify/provide for the training needs of their personnel performing inspections and tests. 

Handling, Storage, Preservation, Packaging, and Shipping . The Contractor shall establish, maintain, control, and be responsible for the procedures for handling, storage, preservation, packaging, and shipping to protect the quality of materials and to prevent damage, loss, deterioration, degradation, or substitution of products.

[bookmark: _Toc119572194]Wood Packing Material
Wood Packaging Material in accordance with ISPM-15, Regulation of Wood Packaging Material in International Trade, is applicable.  Wood packing material includes pallets.  See DLAD T/Q Requirement RP001 DLA Packaging Requirements for Procurement, which includes requirements for treatment of wood packaging material.

[bookmark: _Toc119572195]Military Packaging 
DS7029 and/or DS7033    Preservation, Packing and Marking Instructions

Military Packaging in accordance with MIL-STD-2073-1E is applicable.

	DS7029 - DS7033  LEGEND

	Qty
	Quantity

	Prot Req
	Protection Required

	PKG-REF
	Packaging Reference (Military/Federal Specification or Standard)

	SPI
	Special Packaging Instruction

	LPK
	Level of Packing

	QUP
	Quantity per Unit Pack

	ICQ
	Intermediate Container Quantity

	Pkg Reqmt Codes
	Packaging Requirement Codes when PKG-REF cites MIL-STD-2073

	The below codes are for special markings:

	PC
	Project Code

	WG
	Warranty/Guarantee

	SL
	Shelf Life

	BC
	Bar Code

	FMS
	Foreign Military Sales






	DS7029 - DS7033
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	
	

	NSN
	Prot Req
	PKG-REF or SPI
	LPK
	QUP
	ICQ
	
	
	
	
	
	
	
	
	
	
	
	Special Markings

	
	
	
	
	
	
	Pkg
	J.
	J
	J
	J
	J
	J
	J
	J
	J
	J
	

	
	
	
	
	
	
	Reqmt
	I.
	II.
	III.
	IV.
	V.
	VI.
	VII.
	VII.a
	IX
	X
	

	
	
	
	
	
	
	Codes
	(MP)
	(CD)
	(PM)
	(WM)
	(CD)
	(CT)
	(UC)
	(IC)
	(PK)
	(SM)
	

	6150-12-343-3731
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	NA
	Z
	ED
	00
	Q
	00
	BC

	6150-12-343-3732
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	NA
	Z
	A1
	ED
	Q
	00
	BC

	6150-12-343-3733
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	NA
	Z
	A1
	ED
	Q
	00
	BC

	6150-12-343-3734
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	ZZ
	Z
	A2
	ED
	Q
	00
	BC

	6150-12-343-3735
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	31
	1
	00
	00
	NA
	Z
	BL
	ED
	Q
	00
	BC

	6150-12-343-3736
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	31
	1
	00
	00
	NA
	Z
	BL
	ED
	Q
	00
	BC

	6150-12-343-3737
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	31
	1
	00
	00
	NA
	Z
	BL
	ED
	Q
	00
	BC

	6150-12-343-3738
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	00
	0
	FD
	00
	Q
	00
	BC

	6150-12-343-3739
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	00
	0
	FD
	00
	Q
	00
	BC

	5975-12-343-4086
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	NA
	A
	A2
	ED
	Q
	00
	BC

	5975-12-343-4088
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	10
	1
	00
	00
	NA
	A
	A2
	ED
	Q
	00
	BC

	5975-12-343-4089
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	41
	1
	00
	00
	NA
	D
	ED
	00
	Q
	00
	BC

	8130-12-358-4625
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	41
	1
	00
	00
	NA
	D
	F2
	00
	Q
	00
	BC

	5945-01-577-2614
	Military
	MIL-STD-2073-1E
	B
	001
	
	
	52
	1
	00
	00
	NA
	B
	ED
	00
	Q
	00
	BC
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[bookmark: _Toc119572197]CDRL List
	CDRL Data Line No.
	DID Identification
	Title

	A001
	DI-MISC-
	80711A
	Scientific and Technical Reports – 
IUID Marking Diagram / Instructions

	B001
	DI-PSSS-
	81656B
	Bill of Materials (BOM) for Logistics & Supply Chain Risk Management – Production 



[bookmark: _Toc119572198]Individual CDRLs 
CDRLs are shown starting on the next page.  



	CONTRACT DATA REQUIREMENTS LIST
(1 Data Item)
	Form Approved
OMB No. 0704-0188


	Public reporting burden for this collection of information is estimated to average 110 hours per response, including the time for reviewing instructions, searching existing data sources, gathering and maintaining  the data needed, and completing and reviewing the collection of information. Send comments regarding this burden estimate or any other aspect of this collection of information, including suggestions for reducing this burden, to Department of Defense, Washington Headquarters Services, Directorate for Information Operations and Reports, 1215 Jefferson Davis Highway, Suite 1204, Arlington, VA. 22202-4302, and to the Office of Management and Budget, Paperwork Reduction Project (0704-0188), Washington, DC 20503. Please DO NOT RETURN your form to either of these addresses.  Send completed form to the Government Issuing Contracting Officer for Contract/PR No. listed in Block E.

	A. CONTRACT LINE ITEM NO.
	B.  EXHIBIT
	C.  CATEGORY:

	A001
	
	   TDP      TM      OTHER    MISC   

	D.  SYSTEM/ITEM
	E.  CONTRACT/PR NO.
	F.  CONTRACTOR

	[bookmark: _Hlk246323691]Compoenets for the Electric Power Plant III U/W PATRIOT
	TBD
	TBD

	1. DATA ITEM NO.
	2.  TITLE OF DATA ITEM
	3.  SUBTITLE
	
	17. PRICE GROUP

	
	Scientific and Technical Reports
	[bookmark: OLE_LINK18][bookmark: OLE_LINK19]IUID Marking Diagram/Instructions
	
	

	4. AUTHORITY (Data Acquisition Document No.)
	5. CONTRACT REFERENCE
	6. REQUIRING OFFICE
	
	18. ESTIMATED TOTAL PRICE

	DI-MISC-80711A
	TBD
	FCDD-ISR-HFF
	
	INSERT

	7.  DD 250 REQ
	9.DIST STATEMENT    REQUIRED
	10. FREQUENCY
	12. DATE OF FIRST  SUBMISSION
	14. 	DISTRIBUTION
	
	IN

	DD
	
	ASREQ
	SEE BLOCK 16
	
	b.  COPIES
	
	SECT. B

	8. APP CODE
	N/A
	11. AS OF DATE
	13.  DATE OF SUBSEQUENT
SUBMISSION
	a.   ADDRESSEE
	
Draft
	Final

	A
	
	N/A
	SEE BLOCK 16
	
	
	
Reg
	
Repro

	16. REMARKS:     
     Block 4: Delete Block 10.2 of Data Item Description (DID) and prepare in accordance with the Statement of Work.
     Block 12: Delivery of draft shall be 30 DAC.  Government has 30 days to review/comment.
      Block 13 Delivery of final shall be 30 days after receipt of Government comments.  Government has 30 days to determine acceptance.  Contractor to submit DD250 upon acceptance of UID Marking Diagram/Instructions.
     Block 14:  All digital files will be provided both by electronic submission, e.g., e-mail, FTP, etc., as arranged with the requiring office.

[bookmark: OLE_LINK27][bookmark: OLE_LINK28]If the CDRL Data Deliverable is priced and is not NSP (Not Separately Priced), then an electronic DD Form 250 will be required via the Wide Area Workflow website in order for the contractor to receive payment for the data deliverable (see section G of the Contract). CDRLs that are NSP shall not use WAWF to notify the government. E-mail notification is required with any electronic submission.
	
FCDD-ISR-HFF
	
1
	
1
	
0

	
	15. TOTAL  [image: ]
	1
	1
	0

	G.  PREPARED BY
	H.  DATE
	I.  APPROVED BY
	J.  DATE

	[bookmark: _Hlk222040039]Dave Teicher
FCDD-ISR-HFF
Lead General Engineer
	03/16/26
	

	3/16/26







	CONTRACT DATA REQUIREMENTS LIST
(1 Data Item)
	Form Approved
OMB No. 0704-0188


	Public reporting burden for this collection of information is estimated to average 110 hours per response, including the time for reviewing instructions, searching existing data sources, gathering and maintaining  the data needed, and completing and reviewing the collection of information. Send comments regarding this burden estimate or any other aspect of this collection of information, including suggestions for reducing this burden, to Department of Defense, Washington Headquarters Services, Directorate for Information Operations and Reports, 1215 Jefferson Davis Highway, Suite 1204, Arlington, VA. 22202-4302, and to the Office of Management and Budget, Paperwork Reduction Project (0704-0188), Washington, DC 20503. Please DO NOT RETURN your form to either of these addresses.  Send completed form to the Government Issuing Contracting Officer for Contract/PR No. listed in Block E.

	A. CONTRACT LINE ITEM NO.
	B.  EXHIBIT
	C.  CATEGORY:

	B001
	
	   TDP      TM      OTHER    MISC   

	D.  SYSTEM/ITEM
	E.  CONTRACT/PR NO.
	F.  CONTRACTOR

	Components for the Electric Power Plant III U/W PATRIOT
	TBD
	TBD

	1. DATA ITEM NO.
	2.  TITLE OF DATA ITEM
	3.  SUBTITLE
	
	17. PRICE GROUP

	
	Bill of Materials (BOM) for Logistics & Supply Chain Risk Management
	Production Phase
	
	

	4. AUTHORITY (Data Acquisition Document No.)
	5. CONTRACT REFERENCE
	6. REQUIRING OFFICE
	
	18. ESTIMATED TOTAL PRICE

	DI-PSSS-81656B
	TBD
	FCDD-ISR-HFF
	
	INSERT

	7.  DD 250 REQ
	9.DIST STATEMENT    REQUIRED
	10. FREQUENCY
	12. DATE OF FIRST  SUBMISSION
	14. 	DISTRIBUTION
	
	IN

	DD
	
	BLOCK 16
	60 DAC
	
	b.  COPIES
	
	SECT. B

	8. APP CODE
	N/A
	11. AS OF DATE
	13.  DATE OF SUBSEQUENT
SUBMISSION
	a.   ADDRESSEE
	
Draft
	Final

	A
	
	N/A
	SEE BLOCK 16
	
	
	
Reg
	
Repro

	16. REMARKS:     
The government requires 30 days to provide comments or approve the first submission.  Subsequent semiannual submissions to reflect changes or updates will be submitted 30 days prior to each OWG meeting. Government comments or approval of subsequent submissions will occur concurrent with the OWG minutes.  The contractor needs only to submit data for the following BOM data fields: OEM Part Number, OEM CAGE, Software/Firmware Version (if applicable), Indenture Level, Reference Designator (if assigned), NHA Part Number, NHA CAGE, Nomenclature, NSN (if assigned), Manufacturer's Part Number and Manufacturer's CAGE.  The contractor shall also provide the following additional data fields; "Case Number" (if assigned), "Case Status" (open (being worked); pending approval (submitted to the government for approval); resolved (approved); closed (implemented)), "End of Life (EOL) date".

Note that where the configuration baseline is to government drawings rather than OEM p/n's, then the government drawing numbers & CAGE codes shall be used in lieu of the OEM p/n & CAGE in the BOM.
Submit electronically in Microsoft Excel format (unless otherwise approved by the government)
	
FCDD-ISR-HFF
	
1
	
1
	
0

	
	15. TOTAL  [image: ]
	1
	1
	0

	G.  PREPARED BY
	H.  DATE
	I.  APPROVED BY
	J.  DATE

	Dave Teicher
FCDD-ISR-HFF
Lead General Engineer
	03/16/26
	

	03/6/26
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