Toxic Industrial Chemical/Material Military Exposure Guideline (mg/L) Challenge Concentration (mg/L) 

	Class / Group
	Chemical (CASRN)
	Target influent challenge concentration 
(mg/L ± 20% ) a
	Minimum percent reduction

	inorganic
	arsenic V (pentavalent) (7778-43-0)
	0.6
	≥ 90%

	inorganic
	arsenic III (trivalent) (7778-43-0)
	0.6
	≥ 90%

	inorganic
	cyanide b (143-33-9)
	2
	≥ 90%

	inorganic
	mercury c (7487-84-7)
	0.02
	≥ 90%

	VOC surrogate
	chloroform (67-66-3)
	0.3
	≥ 95%

	gasoline / diesel
	benzene (71-43-2)
	0.05
	≥ 90%

	
	toluene (108-88-3)
	5
	≥ 90%

	
	1,3,5-trimethylbenzene (108-67-8)
	0.06
	≥ 90%

	
	naphthalene (91-20-3)
	0.1
	≥ 90%

	carbamate
	aldicarb (116-06-3)
	0.14
	≥ 90%

	organophosphate
	methamidophos (10265-92-6)
	0.07
	≥ 90%

	herbicide
	paraquat dichloride (1910-42-5)
	0.467
	≥ 90%

	radionuclide
	Uranium  (7440-61-1)
	0.3
	≥ 90%

	dissolved solid
	total dissolved solids  (7647-14-5)
	
	N/A





