Attachment 1: Combined Synopsis-Solicitation for Commercial Products and Commercial Services 
RFQ: 36C24127Q0016 Water Management Program and Chemical Testing

	SUBJECT*
	Water Management Program and Chemical Testing  VAMC Boston Healthcare System 



GENERAL INFORMATION
	CONTRACTING OFFICE’S ZIP CODE*
	04330

	SOLICITATION NUMBER*
	36C24127Q0016

	RESPONSE DATE/TIME/ZONE
	10-30-2026 12:00PM EASTERN TIME, NEW YORK, USA

	ARCHIVE
	7 DAYS AFTER THE RESPONSE DATE

	RECOVERY ACT FUNDS
	N

	SET-ASIDE
	SDVOSBC

	PRODUCT SERVICE CODE*
	F109

	NAICS CODE*
	561210

	CONTRACTING OFFICE ADDRESS
	Department of Veterans Affairs 
Network Contracting Office 1 (NCO 1) 
Contracting Officer (90C) 
1 VA Center
Augusta ME  04330 


	POINT OF CONTACT*


	Contract Specialist 
Pamela L. Parham
pamela.parham3@va.gov
Email Only Please
No Fax Accepted




PLACE OF PERFORMANCE
	ADDRESS
	Department of Veterans Affairs

	
	VAMC Boston Healthcare System

	
	Jamaica Plain, West Roxbury and Brockton Campus

	
	150 South Huntington Avenue

	
	Boston MA

	POSTAL CODE
	02130

	COUNTRY
	USA



ADDITIONAL INFORMATION
	AGENCY’S URL
	https://www.va.gov/boston-health-care/

	URL DESCRIPTION
	VA Boston Healthcare

	AGENCY CONTACT’S EMAIL ADDRESS
	pamela.parham3@va.gov

	EMAIL DESCRIPTION
	Contract Specialist Email




Combined Synopsis/Solicitation Notice
Combined Synopsis/Solicitation Notice
DESCRIPTION
	*= Required Field
	Combined Synopsis/Solicitation Notice
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Description of Services
This is a combined synopsis/solicitation for commercial products and commercial services prepared in accordance with the format Revolutionary FAR Overhaul (RFO) in Federal Acquisition Regulation (FAR) subpart 12.202, “Streamlined Procedures for Evaluation and Solicitation for Commercial Products and Commercial Services,” as supplemented with additional information included in this notice. This announcement constitutes the only solicitation; quotes are being requested, and a written solicitation document will not be issued.

This solicitation is issued as an RFQ.  The solicitation document and incorporated provisions and clauses are those in effect through Federal Acquisition Circular 2026-01. 

This solicitation is set-aside for 100% SDVOSB/VOSB.

The associated North American Industrial Classification System (NAICS) code for this procurement is 561210, with a small business size standard of 19 million. 
The FSC/PSC is F109.

The Network Contracting Office (NCO) 1- New England is seeking a qualified contractor to establish a Water Management Program and provide Water Chemical Testing Services as a Firm-Fixed Price Purchase Order. 

If you have any questions or concerns regarding this solicitation, they should be forwarded in writing via email to the Point of Contact listed below:

Pamela L. Parham              pamela.parham3@va.gov 



All interested companies shall provide quotations for the following:

Supplies/Services

	 
	Products
	 

	Item #
	Description/Part Number*
	Qty
	Unit of Measure
	 Price 
	 Extended Amount 

	001
	Water Management Program and Chemical Testing Services for 3 VA campuses in accordance with the Statement of Work – Base Year

	1
	YR
	
	                                  

	1001
	Water Management Program and Chemical Testing Services for 3 VA campuses in accordance with the Statement of Work- Option Year 1

	1
	YR
	
	                                  

	2001
	Water Management Program and Chemical Testing Services for 3 VA campuses in accordance with the Statement of Work – Option Year 2

	1
	YR
	
	

	3001
	Water Management Program and Chemical Testing Services for 3 VA campuses in accordance with the Statement of Work – Option Year 3 

	1
	YR
	
	 

	4001
	Water Management Program and Chemical Testing Services for 3 VA campuses in accordance with the Statement of Work- Option year 4
	1
	YR
	
	 




(START OF STATEMENT OF WORK)

STERILE PROCESSING SERVICE WATER MANAGEMENT PROGRAM, AND WATER TESTING

General: The Boston VA Medical Center Campus in Boston, MA has a need for the development, testing and maintenance of a water management program, for existing water systems. 

Description of Service: The contractor shall provide all supervision, labor, travel, parts, materials, tool, supplies, and equipment necessary to provide a comprehensive Water Management Program, water testing, and implement a Web-based Data Management System to record, store, and report all data in alignment with AAMI ST-108:2023. On date of award of a contract, the contractor shall take on the full scope of duties, meeting all the requested requirements within the water management services, and water testing/ lab services. Comprehensive Water Management Program Tests shall  be completed within the first 2 weeks of each month.  Water testing shall be conducted monthly, quarterly, and as needed based on re-testing needs due to out-of-range results. 
Period of Performance: The performance period shall be one base year of twelve months, plus four one-year option renewals. 

[image: ]AAMI ST108 Utility Water, Critical Water, and Steam Testing:
[image: ]
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Pre-Work Conference:
Within 10 days after award of the contract, the Contractor shall meet with the designated point of contact to establish mutually agreeable schedules for accomplishment of the required items of work.

Hours of Operation
Water testing shall be done during normal business hours of 0730-1600, Monday through Friday.  


Water Management Services

Water Management Development for Sterile Processing Service
The contractor shall develop a Water Management Program (WMP) for the sterile processing service (SPS) water systems in alignment with VA and industry standards, including the following:
• AAMI ST-108:2023 Water for the processing of Medical Devices
• Association of perioperative Registered Nurses (AORN) Guideline for Cleaning and
Care of Surgical Instruments
• VHA Directive 1116(2) Sterile Processing Services (SPS)

The water management program shall contain the following elements for water safety:
• Program Team (Water Management Team) – Identify persons responsible for SPS
WMP development, implementation, and operation.
• Develop Program Goals – Establish water safety and quality goals for SPS.
• Describe Water Systems – Describe the critical water, utility water, and steam systems within SPS and develop water-system process flow diagrams.
• Analysis of Building Water Systems – Conduct a systematic analysis of hazardous
conditions in the SPS water systems.
• Control Locations – Determine the locations in the system where control measures are required.
• Control Limits – For each control measure at each control location established,
determine the limits including but not limited to a maximum value, a minimum value, or a range of values within which a chemical or physical parameter must be monitored and
maintained to reduce hazardous conditions to an acceptable level.
• Control Measures – Outline the means, methods, or procedures used to maintain
the physical or chemical conditions of water to within control limits.
o Routine preventative maintenance program for the critical water system.
o Flushing program for both critical and utility/potable water during times of low water usage in SPS.
• Monitoring – Establish procedures for monitoring whether control measures are
operating within established control limits.
• Corrective Actions – Establish the corrective actions to be taken when monitoring
indicates that the control parameters are outside of the established control limits.
• Develop Verification Strategy – Establish procedures to confirm that all the program

elements are being implemented as designed at a frequency established by the WMT.
• Develop Validation Strategy – Establish additional, outside of baseline stated in above chart (AAMI ST108 Utility Water, Critical Water, and Steam Testing), validation criteria and frequency to confirm that the program effectively controls the hazardous conditions throughout the SPS water
systems.
• Documentation – Establish documentation and communication procedures for all
activities of the WMP and maintain records appropriate to these principles and their
application.
Water Management Program Operations for Sterile Processing Service
Upon completion and approval of the Water Management Program (WMP), the contractor shall provide WMP operation services in support of the Water Management Team (WMT) for the facility’s SPS water systems. The WMP operation services shall contain the following elements for water safety:
• Facilitate quarterly meetings for the Water Management Team.
• Maintain, assist, and advise in the operation of the WMP and generate required
documentation.
• Recommend and implement changes to the WMP as directed by the Water
Management Team to achieve the desired performance in alignment with AAMI ST-108:2023 and VHA Directive 1116(2).
• Provide, operate, and continue to customize the WMP using the web-based data
management software.
• Provide remote support on water management questions as needed.
• Provide training to the Water Management Team on the WMP process and best
practices for SPS water systems.
• Verify that the WMP is being implemented as designed on a quarterly basis through
monitoring and documentation of system performance and WMP records and record in
the web-based data management software.
• Validate that the WMP adequately controls the hazardous conditions in the building
water system through the review of on-site water testing.

Web based Data Management System
The existing web-based data management systems used to collect, report, and store continuous monitoring water data will be used for WMP development and operations. The web-based data management system shall provide the following functions:

• All information stored in the system is available 24/7 via password protected access
• WMP-related reports (including validation testing results, meeting minutes, verification
reports, and service provider reports) can be stored and available for immediate access by all users
• Customized charts, reports, views, and data entry screens as requested
• Management dashboards with industry benchmarking
• Send text or email alerts for data that is outside of set parameters
• Automated data collection via continuous monitoring equipment (equipment not included)

• Validation test results immediately uploaded 
• Exportable data to excel and other formats

The purchase order’s period of performance is estimated to start in April 2026 – April 2027. The period of performance shall be for one base year of 12 months with 4 twelve month option periods, for a total of five years. 

Place of Performance/Place of Delivery
Jamaica Plain VA Medical Center
150 South Huntington Avenue
Boston, MA 02130-4817

West Roxbury VA Medical Center
1400 VFW Parkway
West Roxbury, MA 02132-4927

Brockton VA Medical Center
940 Belmont Street
Brockton, MA 02301-5596

(END OF STATEMENT OF WORK)

(START OF PROVISIONS)

The full text of FAR provisions or clauses may be accessed electronically at https://www.acquisition.gov/browse/index/far. 

The following solicitation provisions and clauses apply to this acquisition:
1. FAR 52.212-1, Instructions to Offerors-Commercial Products and Commercial Services (SEP 2023) (DEVIATION OCT 2025)
All quoters shall submit the following: Price, Technical, and Past Performance. 
a. Page 3 of this Combined Synopsis/Solicitation with the price and total filled out.
b. Cost Breakdown of vendor price
c. Provide SDVOSB certification from SBA.gov.
d. Provide past performance with minimum of three references.
e. Provide documentation to demonstrate Water Management Program Technical Approach, Qualifications, Experience, and Lab Capabilities. 
f. Provide a capability statement for Independence, Accreditation and Laboratory Proximity and Redundancy.
g. Provide a statement for On-site Personnel and Reporting Capabilities.
h. Provide filled out and signed VAAR 852.219-75. 

All quotes shall be sent to the Contract Specialist, Pamela L. Parham, pamela.parham3@va.gov. 

Award will be based upon a comparative evaluation of quotes in accordance with the Simplified Acquisition Procedures of RFO FAR 12. Comparative evaluation is the side by side pairwise comparison of quotes based on factors resulting in a Contracting Officer decision for the quote most favorable to the Government.	

2. www.sam.gov registration is required to be complete at time of submission of response. Offerors must complete annual representations and certifications electronically via the System for Award Management (SAM) website located at https://sam.gov/.

3. FAR 52.212-4, Contract Terms and Conditions-Commercial Products and Commercial Services (NOV 2023) (DEVIATION OCT 2025) 

4. FAR 52.252-1, Solicitation Provisions Incorporated by Reference (FEB 1998) - This solicitation incorporates one or more solicitation provisions by reference, with the same force and effect as if they were given in full text. Upon request, the Contracting Officer will make their full text available. The offeror is cautioned that the listed provisions may include blocks that must be completed by the offeror and submitted with its quotation or offer. In lieu of submitting the full text of those provisions, the offeror may identify the provision by paragraph identifier and provide the appropriate information with its quotation or offer. Also, the full text of a solicitation provision may be accessed electronically at this/these address(es): https://www.acquisition.gov/far-overhaul/far-part-deviation-guide/far-overhaul-part-52#FAR_52_252_1 (FAR) and http://www.va.gov/oal/library/vaar/index.asp (VAAR)
5. ADDENDUM to FAR 52.212-2 EVALUATION—COMMERCIAL PRODUCTS AND COMMERCIAL SERVICES (DEVIATION AUG 2025)
(a) The following factors shall be used to evaluate quotations: 
(1)     Technical or Quality: The offeror’s quote shall be evaluated to determine if the   contractor has the experience and capabilities to provide quality services in a timely and efficient manner. 
(a) Water Management Program Development & Technical Approach – Contractor shall demonstrate thorough understanding of AAMI ST-108, covering hazard analysis, control limits/measures, monitoring, corrective actions, and verification/validation strategy. 
(b) Qualifications, Experience and Lab Capabilities – The Government will assess the Offeror’s ability to provide independent, accredited, and reliable SPS‑focused water testing services. Evaluation will consider:
(c) Independence
Clear demonstration of no conflict of interest, including no sale of treatment chemicals or devices.
(d) Accreditation
Current EMLAP, NELAP, or equivalent state accreditation covering all required ST‑108 analytes.
(e) Laboratory Proximity
A primary testing lab located near Boston to minimize sample degradation and transit delays.
(f) Dedicated On‑Site Personnel
Employee assigned to perform monthly on‑site testing to ensure continuity and consistency.
(g) Laboratory Redundancy
Access to multiple laboratories capable of processing samples to ST‑108 standards in case of emergent need.
(h) Summary Reporting Capability
Ability for all laboratories to produce single‑page summary reports listing all biological and chemical analytes with corresponding ST‑108 maximum concentration levels.
(i) Contractor will provide a quality control plan, which explains the offerors approach to quality control and methodologies. 
(j)  If you are planning to sub-contract some or all of this work, please provide the name and address(s) of all subcontractor(s) (if applicable) and a description of their planned subcontracting effort.
(2) Past Performance:
(a) Provide (3) references of work, similar in scope and size with the requirement detailed in the Performance Work Statement.  Refer to Past Performance sheet in section D.  References must include contact information, brief description of the work completed, and contract # (if relevant).  References may be checked by the Contracting Officer to ensure your company has complied with prior requirements, responded to issues and performed in accordance with the PWS. 
(b) Past performance information may also be obtained from other sources available to the Government to include, but not limited to, Contractor Performance Assessment Reporting System (CPARS), System for Award Management (SAM), or other databases.
(3) Veterans Involvement: 
(a) SDVOSBs and VOSBs must be registered and certified in the Small Business Administration Small Business Search (SBA DSBS) database (https://search.certifications.sba.gov).
(4) Price: Complete line items on Page 2 of this combined synopsis/solicitation, which will be completed by the offeror.
(b) Evaluation Approach. The Government will evaluate quotations using the comparative evaluation process outlined in FAR 13.106-2 (b) (3), where quotations will be compared to one another to determine which provides the best benefit to the Government. The Government reserves the right to consider a quotation other than the lowest price that provides additional benefit(s). Quotations may exceed minimum requirements of the solicitation. The Government reserves the right to select a quotation that provides benefit to the Government that exceeds the minimum requirements of the solicitation but is not required to do so. Each response must meet the minimum requirements of the solicitation. The Government is not requesting or accepting alternate quotations. The evaluation will consider the following: 
(1) Technical or Quality: The quotation will be evaluated to the extent to which it can meet and/or exceed the Government’s requirements as outlined in the solicitation and based on the information requested in the instructions to quoters section of the solicitation.
(2) Past Performance: The past performance evaluation will assess the relative risks associated with a quoter’s likelihood of success in fulfilling the solicitation’s requirements as indicated by the quoter’s record of past performance. The past performance evaluation may be based on the contracting officer’s knowledge of and previous experience with the supply or service being acquired; Customer surveys, and past performance questionnaire replies; Contractor Performance Assessment Reporting System (CPARS) at http://www.cpars.gov/;   or any other reasonable basis.
(3) Veterans Involvement: In accordance with Veterans Affairs Acquisition Regulation (VAAR) 852.215-70 (DEVIATION), Service-Disabled Veteran-Owned and Veteran-Owned Small Business (VOSB) Evaluation Factors, the Government will assign evaluation credit for a Quoter (i.e., prime contractor) which is a Service-Disabled Veteran-Owned Small Business (SDVOSB) or a VOSB.  To receive credit, an offeror must be registered and verified in Small Business Administration Small Business Search (SBA DSBS) database (https://search.certifications.sba.gov) at time of quotation submission and at time of award and must meet federal small business size standards for the North American Industry Classification System (NAICS) code assigned to this solicitation. Non-SDVOSB/VOSB quotations that use SDVOSBs or VOSBs as subcontractors will receive some consideration under this evaluation Factor. Quoters must state in their quotations the names of the SDVOSBs and VOSBs with whom they intend to subcontract and provide a brief description of the proposed subcontracts and the approximate dollar values of the proposed subcontracts. In addition, the proposed subcontractors must be registered and verified in the SBA DSBS and must meet federal small business size standards for the NAICS code assigned to this solicitation at time of both quotation submission and at time of award.
(4) Price: The Government will evaluate the price by adding the total of all line-item prices. The Total Evaluated Price will be that sum.
6. FAR 52.203-18, Prohibition on Contracting with Entities that Require Certain Internal Confidentiality Agreements or Statements-Representation. (JAN 2017)
7. FAR 52.204-7, System for Award Management—Registration (NOV 2024) (DEVIATION NOV 2025)
8. FAR 52.222-18, Certification Regarding Knowledge of Child Labor for Listed End Products.(FEB 2021)
(END OF PROVISIONS)

(START OF CLAUSES)

9. FAR 52.252-2, Clauses Incorporated by Reference (FEB 1998) - This contract incorporates one or more clauses by reference, with eh same force and effect as if they were given in full text. Upon request, the Contracting Officer will make their full 
10. text available. Also, the full text of a clause may be accessed electronically at this/these address(es):
http://www.acquisition.gov/far/index.html (FAR) and
http://www.va.gov/oal/library/vaar/index.asp (VAAR)
11. FAR 52.203-17, Contractor Employee Whistleblower Rights. (NOV 2023)
12. FAR 52.203-19, Prohibition on Requiring Certain Internal Confidentiality Agreements or Statements. (JAN 2017)
13. FAR 52.204-9, Personal Identity Verification of Contractor Personnel (JAN 2011)
14. FAR 52.204-13, System for Award Management-Maintenance (OCT 2018) (DEVIATION NOV 2025)
15. FAR 52.209-6, Protecting the Government's Interest When Subcontracting With Contractors Debarred, Suspended, Proposed for Debarment, or Voluntarily Excluded. (JAN 2025) (DEVIATION NOV 2025)
16. FAR 52.209-10, Prohibition on Contracting With Inverted Domestic Corporations. (NOV 2015) (DEVIATION NOV 2025)
17. FAR 52.219-14, Limitations on Subcontracting. (OCT 2022) (DEVIATION NOV 2025)
18. FAR 52.222-3, Convict Labor. (JUN 2003) (DEVIATION NOV 2025)
19. FAR 52.222-19, Child Labor-Cooperation with Authorities and Remedies. (JAN 2025) (DEVIATION NOV 2025)
20. FAR 52.222-36, Equal Opportunity for Workers with Disabilities. (JUN 2020) (DEVIATION NOV 2025)
21. FAR 52.222-41, Service Contract Labor Standards. (AUG 2018) (DEVIATION NOV 2025)
22. FAR 52.222-42, Statement of Equivalent Rates for Federal Hires. (MAY 2014)
23. FAR 52.222-43, Fair Labor Standards Act and Service Contract Labor Standards-Price Adjustment (Multiple Year and Option Contracts). (AUG 2018) (DEVIATION NOV 2025)
24. FAR 52.222-50, Combating Trafficking in Persons. (NOV 2021) (DEVIATION NOV 2025)
25. FAR 52.222-62, Paid Sick Leave Under Executive Order 13706. (JAN 2022) (DEVIATION NOV 2025)
26. FAR 52.223-23, Sustainable Products. (MAY 2024) (DEVIATION NOV 2025)
27. FAR 52.226-8, Encouraging Contractor Policies to Ban Text Messaging While Driving. (MAY 2024)
28.  FAR 52.232-33, Payment by Electronic Funds Transfer-System for Award Management. (OCT 2018)
29.  FAR 52.233-3, Protest after Award. (AUG 1996) (DEVIATION NOV 2025)
30.  FAR 52.233-4, Applicable Law for Breach of Contract Claim. (OCT 2004) (DEVIATION NOV 2025)
31.  FAR 52.240-91, Security Prohibitions and Exclusions. (DEVIATION NOV 2025)
32.  FAR 52.244-6, Subcontracts for Commercial Products and Commercial Services. (JAN 2025) (DEVIATION OCT 2025)
33. FAR 52.222-14, Disputes Concerning Labor Standards (FEB 1988) (DEVIATION NOV 2025)
34.  FAR 52.222-15, Certification of Eligibility (MAY 2014)
35.  FAR 52.222-55, Minimum Wages for Contractor Workers Under Executive Order 14026 (JAN 2022) (DEVIATION NOV 2025)
36. FAR 52.223-5, Pollution Prevention and Right-to-Know Information (MAY 2024)
37.  FAR 52.252-6, Authorized Deviations in Clauses (NOV 2020) - (b) The use in this solicitation or contract of any VA Acquisition Regulation (VAAR) and 48 CFR Chapter 8 clause with an authorized deviation is indicated by the addition of "(DEVIATION)" after the name of the regulation.
38.  VAAR 852.209-70, Organizational Conflicts of Interest (OCT 2020)
39.  VAAR 852.203-70, Commercial Advertising (MAY 2018)
40.  VAAR 852.204-70, Personal Identity Verification of Contractor Personnel (MAY 2020)
41.  VAAR 852.219-73, VA Notice to Total Set-Aside for Certified Service-Disabled Veteran-Owned Small Businesses (JAN 2023) (DEVIATION)
42. VAAR 852.219-74, VA Notice to Total Set-Aside for Certified Veteran-Owned Small Businesses (JAN 2023) (DEVIATION)
43.  VAAR 852.232-72, Electronic Submission of Payment Requests (NOV 2018)
44. VAAR 852.239-76 Information and Communication Technology Accessibility 
45. VAAR clause 852.240‑70, Compliance with P.L. 119‑37 § 258 (DEVIATION) (Mar 2026)
46.  VAAR 852.242-71, Administrative Contracting Officer (OCT 2020)


(END OF CLAUSES AND PROVISIONS)


To facilitate the award process, all quotes must include a statement regarding the terms and conditions herein as follows:
"The terms and conditions in the solicitation are acceptable to be included in the award document without modification, deletion, or addition."
Quoters shall list exception(s) and rationale for the exception(s), if any.

Submission of your response shall be received not later than 10/30/2026 at 12:00PM EST. and email sent to Pamela.Parham3@va.gov.  Any questions shall be received no later than 10/16/2026 at 12:00PM EST.

Late submissions shall be treated in accordance with the solicitation provision at FAR 52.212-1(f). Not Accepted.

Any questions or concerns regarding this solicitation should be forwarded in writing via e-mail to the Point of Contact listed below: Pamela L. Parham   pamela.parham3@va.gov 
852.219-75  VA NOTICE OF LIMITATIONS ON SUBCONTRACTING—CERTIFICATE OF COMPLIANCE FOR SERVICES AND CONSTRUCTION (JAN 2023) (DEVIATION)
  (a) Pursuant to 38 U.S.C. 8127(l)(2), the offeror certifies that—
    (1) If awarded a contract (see FAR 2.101 definition), it will comply with the limitations on subcontracting requirement as provided in the solicitation and the resultant contract, as follows:
      (i) [] Services. In the case of a contract for services (except construction), the contractor will not pay more than 50% of the amount paid by the government to it to firms that are not certified SDVOSBs listed in the SBA certification database as set forth in 852.219–73 or certified VOSBs listed in the SBA certification database as set forth in 852.219–74. Any work that a similarly situated certified SDVOSB/VOSB subcontractor further subcontracts will count towards the 50% subcontract amount that cannot be exceeded. Other direct costs may be excluded to the extent they are not the principal purpose of the acquisition and small business concerns do not provide the service as set forth in 13 CFR 125.6.
      (ii) [] General construction. In the case of a contract for general construction, the contractor will not pay more than 85% of the amount paid by the government to it to firms that are not certified SDVOSBs listed in the SBA certification database as set forth in 852.219–73 or certified VOSBs listed in the SBA certification database as set forth in 852.219–74. Any work that a similarly situated certified SDVOSB/VOSB subcontractor further subcontracts will count towards the 85% subcontract amount that cannot be exceeded. Cost of materials are excluded and not considered to be subcontracted.
      (iii) [] Special trade construction contractors. In the case of a contract for special trade contractors, the contractor will not pay more than 75% of the amount paid by the government to it to firms that are not certified SDVOSBs listed in the SBA certification database as set forth in 852.219–73 or certified VOSBs listed in the SBA certification database as set forth in 852.219–74. Any work that a similarly situated certified SDVOSB/VOSB subcontractor further subcontracts will count towards the 75% subcontract amount that cannot be exceeded. Cost of materials are excluded and not considered to be subcontracted.
    (2) The offeror acknowledges that this certification concerns a matter within the jurisdiction of an Agency of the United States. The offeror further acknowledges that this certification is subject to Title 18, United States Code, Section 1001, and, as such, a false, fictitious, or fraudulent certification may render the offeror subject to criminal, civil, or administrative penalties, including prosecution.

    (3) If VA determines that an SDVOSB/ VOSB awarded a contract pursuant to 38 U.S.C. 8127 did not act in good faith, such SDVOSB/VOSB shall be subject to any or all of the following:
      (i) Referral to the VA Suspension and Debarment Committee;
      (ii) A fine under section 16(g)(1) of the Small Business Act (15 U.S.C. 645(g)(1)); and
      (iii) Prosecution for violating 18 U.S.C. 1001.
  (b) The offeror represents and understands that by submission of its offer and award of a contract it may be required to provide copies of documents or records to VA that VA may review to determine whether the offeror complied with the limitations on subcontracting requirement specified in the contract. Contracting officers may, at their discretion, require the contractor to demonstrate its compliance with the limitations on subcontracting at any time during performance and upon completion of a contract if the information regarding such compliance is not already available to the contracting officer. Evidence of compliance includes, but is not limited to, invoices, copies of subcontracts, or a list of the value of tasks performed.
  (c) The offeror further agrees to cooperate fully and make available any documents or records as may be required to enable VA to determine compliance with the limitations on subcontracting requirement. The offeror understands that failure to provide documents as requested by VA may result in remedial action as the Government deems appropriate.
  (d) Offeror completed certification/fill-in required. The formal certification must be completed, signed and returned with the offeror’s bid, quotation, or proposal. The Government will not consider offers for award from offerors that do not provide the certification, and all such responses will be deemed ineligible for evaluation and award.
Certification
I hereby certify that if awarded the contract, [insert name of offeror] will comply with the limitations on subcontracting specified in this clause and in the resultant contract. I further certify that I am authorized to execute this certification on behalf of [insert name of offeror].
[bookmark: _Hlk125346837]Printed Name of Signee: _________________________________________
Printed Title of Signee: ___________________________________________
Signature: _____________________________________________________
Date: _________________________________________________________
Company Name and Address: ______________________________________
_______________________________________________________________
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Location: Jamaica Plain 

Campus

Utility Water 

Quality 

Measurement

Units

Utility Water 

Requiremen

ts

Utility Testing 

Frequency

pH n/a 5.0-7.5 Monthly

Total Alkalinity

mg 

CaCO3/L

<8 Monthly

Conductivity 

uSiemens/c

m

<10 Monthly

Total Hardness

mg 

CaCO3/L

<1 Monthly

Heterotrophic 

Plate Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

Heterotrophic 

Plate Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

pH n/a 6.5-9.5 Monthly

Total Alkalinity

mg 

CaCO3/L

<400 Monthly

Conductivity 

uSiemens/c

m

<500 Monthly

Total Hardness

mg 

CaCO3/L

<150 Monthly

Heterotrophic 

Plate Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity

mg 

CaCO3/L

<400 Quarterly

Conductivity 

uSiemens/c

m

<500 Quarterly

Total Hardness

mg 

CaCO3/L

<150 Quarterly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity

mg 

CaCO3/L

<400 Quarterly

Conductivity 

uSiemens/c

m

<500 Quarterly

Total Hardness

mg 

CaCO3/L

<150 Quarterly

Heterotrophic 

Plate Count

CFU/mL <500 Quarterly

Utility water at Scope 

room decon sink 2, 

Ultrasonic 1 & 2, and 

Decon sink 1,2,3 in 

endoscopy suite (MB-

2570)

Heterotrophic 

Plate Count

CFU/mL <500 Quarterly

pH n/a 5.0-9.2 Quarterly

Total Alkalinity

mg 

CaCO3/L

<8 Quarterly

Conductivity 

uSiemens/c

m

<10 Quarterly

Total Hardness

mg 

CaCO3/L

<1 Quarterly

Critical Point of 

Generation, RO Return 

Loop and Decon Sink 1 in 

Decon Area(WC-5220)

Critical water at  Washer 

Disinfector 1 and scope 

room decon sink 2  (MB-

3330)

Medivators 1-8 in 

endoscopy suite(WC-

5140)

Utility Point of Generation 

(WC-5120)

Utility Water at  decon 

sink 1 (WC-5130)

Steam (WC-5300)


image1.emf
Location: Brockton Campus

Utility Water 

Quality 

Measurement

Units

Utility Water 

Requirements

Utility 

Testing 

Frequency

pH n/a 5.0-7.5 Monthly

Total Alkalinity mg CaCO3/L <8 Monthly

Conductivity  uSiemens/cm <10 Monthly

Total 

Hardness

mg CaCO3/L <1 Monthly

Heterotrophic 

Plate Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

Heterotrophic 

Plate Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity mg CaCO3/L <400 Quarterly

Conductivity  uSiemens/cm <500 Quarterly

Total 

Hardness

mg CaCO3/L <150 Quarterly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity mg CaCO3/L <400 Quarterly

Conductivity  uSiemens/cm <500 Quarterly

Total 

Hardness

mg CaCO3/L <150 Quarterly

Heterotrophic 

Plate Count

CFU/mL <500 Quarterly

Utility water at Ultrasonic and Eye Room Decon 

Sink (MB-2570)

Heterotrophic 

Plate Count

CFU/mL <500 Quarterly

pH n/a 5.0-9.2 Quarterly

Total Alkalinity mg CaCO3/L <8 Quarterly

Conductivity  uSiemens/cm <10 Quarterly

Total 

Hardness

mg CaCO3/L <1 Quarterly

Critical Point of Generation, RO Return Loop 

and 2 basin Decon Sink in Building 32 basement 

(WC-5220)

Critical water at  Washer Disinfector 1 and Eye 

Room Decon Sink  (MB-3330)

Utility Point of Generation (WC-5120)

Utility Water at 2 basin decon sink in basement 

(WC-5130)

Steam (WC-5300)
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Location: West Roxbury 

Campus

Utility Water 

Quality 

Measurement

Units

Utility Water 

Requirements

Utility 

Testing 

Frequency

pH n/a 5.0-7.5 Monthly

Total Alkalinity mg CaCO3/L <8 Monthly

Conductivity 

uSiemens/c

m

<10 Monthly

Total Hardness mg CaCO3/L <1 Monthly

Heterotrophic Plate 

Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

Heterotrophic Plate 

Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

pH n/a 6.5-9.5 Monthly

Total Alkalinity mg CaCO3/L <400 Monthly

Conductivity 

uSiemens/c

m

<500 Monthly

Total Hardness mg CaCO3/L <150 Monthly

Heterotrophic Plate 

Count

CFU/mL <10 Monthly

Endotoxin EU/mL <10 Monthly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity mg CaCO3/L <400 Quarterly

Conductivity 

uSiemens/c

m

<500 Quarterly

Total Hardness mg CaCO3/L <150 Quarterly

pH n/a 6.5-9.5 Quarterly

Total Alkalinity mg CaCO3/L <400 Quarterly

Conductivity 

uSiemens/c

m

<500 Quarterly

Total Hardness mg CaCO3/L <150 Quarterly

Heterotrophic Plate 

Count

CFU/mL <500 Quarterly

Utility water at basement 

Decon Sink 2 &3, Belimed 

ultrasonic, Sink 1 and 2 

from medivator room, 

TEE machine, and Sink 

from C1-3A scope room 

(MB-2570)

Heterotrophic Plate 

Count

CFU/mL <500 Quarterly

pH n/a 5.0-9.2 Quarterly

Total Alkalinity mg CaCO3/L <8 Quarterly

Conductivity 

uSiemens/c

m

<10 Quarterly

Total Hardness mg CaCO3/L <1 Quarterly

Critical Point of 

Generation, RO Return 

Loop and Decon Sink 1 A-

B1G(WC-5220)

Critical water at  Washer 

Disinfector 1 and Decon 

sink in Medivator room 

(MB-3330)

Medivators 26-29 in 

medivator room and 

Medivators 1-4 in C1-3A 

scope room (WC-5140)

Utility Point of Generation 

(WC-5120)

Utility Water at basement  

decon sink 1(WC-5130)

Steam (WC-5300)


