


[bookmark: _Toc233282418]Bureau of International Narcotics and Law Enforcement Affairs (INL)
Weapons Program Mexico
Statement of Work
IT EQUIPMENT
1. GENERAL 
The Bureau of International Narcotics and Law Enforcement Affairs (INL) leads the Department of State’s anticrime and counter-narcotics efforts. INL’s mission is to minimize the impact of international crime and illegal drugs on the United States, its citizens, and partner nations by providing effective foreign assistance and fostering global cooperation. INL supports our partner nations on stabilization and strengthening of security institutions to build a global security capacity for combating drug trafficking and other transnational crimes such as money laundering and criminal gangs. INL also provides assistance on strengthening of justice sector institutions, which fosters promotion of good governance and respect for human rights.  
2. [bookmark: _Toc233282419][bookmark: _Hlk65680935]SCOPE 
With support from the Bureau of International Narcotics and Law Enforcement Affairs (INL), specialized equipment and software will be procured.
3. [bookmark: _Toc233282420]REQUIREMENTS
3.1 The Contractor shall acquire and deliver new software and IT equipment, as described in Appendix A - Software and IT Equipment (Technical Specifications of Items) to the U.S. Government (USG) for the benefit of the Government of Mexico (GOM) at INL Warehouse in Brownsville, see section 5, Table One - Delivery Location. The contractor shall provide an OEM in-country warranty valid and applicable in Mexico for all equipment listed in Appendix A. All goods shall be new, must arrive without damage and shall meet or exceed the salient characteristics as detailed. Refurbished, recycled or used items are not acceptable. No installation is required.

3.2 Contractor shall coordinate the delivery with INL logistics point of contact at any time. Contractor must wait to receive INL written confirmation before delivering any item/equipment. The Contracting Officer (CO), the Contracting Officer Representative (COR), the Government Technical Monitor (GTM), the Strategic Acquisition Planning (SAP) Team and INL Weapons Program must always be copied in all communication.

3.3 All items shall be received by INL Logistics/Weapons Program/COR-GTM/SAP team at the INL Warehouse in Brownsville. It is critical that the contractor ensure pallets are packed and organized strictly by end user — no mixed merchandise between end users will be accepted. The equipment shall be organized and labeled by the contractor per end user: CBP-CAMDEX, FBI-TEDAC1 and FBI-TEDAC2 as described in Appendix One. Once received, the USG will inventory the items and reseal the boxes with contractor support. INL Mexico will be responsible for transporting the equipment from Brownsville to the INL warehouse in Mexico. Each end user will then be responsible for distributing their respective items to their final destination.

3.4 For the delivery of the software licenses, vendor shall provide a link per end user to download them along with written instructions for their installation. The vendor shall coordinate with INL Logistics to obtain the appropriate Point of Contact (POC) information under which the licenses will be registered. Final users will install software by themselves so periods of validity of the licenses must begin once final users are able to install the software on their computer equipment. Contractor shall ensure that validity period does not begin before this. Contractor shall be able to provide technical support via email or phone call in case it is required by end users when they are doing the installation. Detailed written instructions shall be provided as well so end users can install the licenses by themselves.

3.5 Partial deliveries are not allowed. The Contractor is required to have a physical representative on site during the delivery and for the duration of inspection by the Government or its agents. The Government intends to open boxes for a complete physical inspection of all delivered equipment and encourages the Contractor to consider the best way to deliver the equipment in a way that facilitates inspection. The Contractor shall be responsible for loading and unloading all items at the warehouse in an organized manner, sorted by end user. Any handling, staging, and arrangement of equipment within the delivery area and inventory shall be performed by the Contractor's on-site representative to ensure proper identification and accountability of all delivered items.

3.6 Upon contract award, the contractor shall schedule and conduct a virtual kickoff meeting within five (5) calendar days. This upcoming meeting will bring together the GTM, INL SAP Team, Weapons Program team, Logistics team, the CO and the COR, as well as representatives from the CBP and FBI. Its purpose is to clarify the scope of work, set main points of contact, and confirm the delivery schedule.

3.7 Note: A donation process to the GOM is not required for this delivery, as the USG will be the recipient.
4. [bookmark: _Toc233282421]PERIOD OF PERFORMANCE
4.1 Contractor shall complete delivery within a period of 60 calendar days after Contract is awarded for all items listed in Appendix A.

4.2 Interim Secure Storage may be required prior to shipping the items to the designated location listed in Section 5, Table One – Delivery Location, this storage may last up to 60 calendar days. 
5. [bookmark: _Toc233282422]DELIVERY
5.1 No item (hardware and software) can be delivered at final destination without previous authorization and coordination with INL Mexico Logistics, and INL Weapons Program. Contractor must wait to receive INL confirmation before delivering equipment. Once the Contractor gets written approval, a specific delivery date will be established. Any action taken from contractor without writing confirmation will be considered under clause Nonpayment for unauthorized work.

5.2 Contractor must ensure all items are prepared for safe transportation once confirmation from INL Logistics and Weapons Program is received. Contractor will be responsible for unloading. The Contractor shall replace lost or damaged items during transportation and/or unloading. Contractor’s personnel must be present at the time of delivery to conduct the inventory of all the items listed in Appendix A.

5.3 All delivery information, including the packing list and a Technical Specifications/Data sheet of all IT equipment and software shall be forwarded to INL Weapons Program and INL Mexico Logistics (mexicocityinllogistics@groups.state.gov) two (2) weeks in advance of delivery to the delivery location detailed in this section Table One. See section 7, Table Two –Deliverables List. The packing list shall include but not limited to: Item Description, Name of Manufacturer, Model Number, Serial Numbers, Delivered Quantity, Unit Price, Extended Price, and Warranty Expiration Date for all hardware. 

5.4 One copy of the packing list must accompany the delivery. The packing list shall be attached to the outside of the "lead" or number one box/carton/package or individually attached to the outside of each box/carton/package.

Table One – Delivery Location
	Country 
	Location

	United States
	225 South Vermillion Rd., Brownsville, TX., 78521
POC Laura Cisneros, CisnerosLL@state.gov



5.5 INL will be responsible for transporting the equipment from Brownsville to the INL warehouse in Mexico. End users will be responsible for deploying and installing, as required.
6. [bookmark: _Toc233282423]IN-COUNTRY WARRANTY
6.1 The Contractor shall provide two years in-country warranty valid ad applicable in Mexico for the hardware listed in Appendix A. Equipment shall be delivered and maintained in good condition and will be inspected upon receipt at the warehouse in Brownsville, Texas. If any equipment is found to be damaged, defective, or not in acceptable condition, it will be returned to the vendor for correction or replacement.

6.2 The OEM warranty shall commence upon delivery of the equipment in Brownsville.

6.3 The contractor shall, confirm for each hardware item listed in Appendix A whether it includes a valid in-country warranty applicable in Mexico. 

6.4 Warranty clause applicable in Mexico remains unchanged and is included as a mandatory requirement. Due to the sensitive nature of the IT equipment, no modifications, substitutions, or exceptions to the warranty requirements will be accepted. 
7. [bookmark: _Toc233282424]DELIVERABLES
7.1 The contractor shall provide the original hard copy and a PDF copy of the Technical Data Sheet in English for all equipment and software listed in Appendix A. See below Table Two – Deliverables List.

7.2 The contractor shall provide the original hard copy and a PDF copy of the Manuals in English for all equipment, and software listed in Appendix A. See below Table Two – Deliverables List.

[bookmark: _Hlk107222391][bookmark: _Hlk89872656]7.3 The contractor shall provide both the original hard copy and a PDF copy of the in-country warranty documentation in English for all equipment listed in Appendix A. The contractor shall ensure hard copies are included with the equipment at the time of delivery. In country warranty must include the expiration date.  See below Table Two – Deliverables List.
Table Two – Deliverables List

	Deliverable
	Language
	Due Date
	Distribution

	D01 A packing list. Pdf format
	English
	Fourteen calendar days prior to delivery.
	INL Logistics
INL SAP team
INL Weapons Program 
GTM/COR

	D02 Technical Data Sheet for equipment listed in Appendix A. Pdf format.
	English
	Fourteen calendar days prior to delivery.
	INL Logistics
INL SAP Team
INL Weapons Program
GTM

	D04 Manuals for equipment & software listed in Appendix A. The original hard copy and a Pdf copy.
	English
	Hard copy shall be included with the equipment at the time of delivery.
Pdf copies no later than seven calendar days after delivery.
	Hard Copy to End User.
A pdf copy to INL SAP team, GTM & INL Weapons Program

	D03 In-Country  warranty for equipment listed in Appendix A. The original hard copy and a Pdf copy.
	English 
	Hard copy shall be included with the equipment at the time of delivery.
Pdf copies no later than seven calendar days after delivery.
	Hard Copy to End User.
A pdf copy to INL SAP team, GTM & INL Weapons Program



7.4 All deliverables shall include a cover page incorporating at least the following information:

· Deliverable number and name
· Contract number
· Project title
· Date of submission
· Document version number
· Contractor’s Name


[bookmark: _Toc233282426]APPENDIX A – SOFTWARE AND IT EQUIPMENT
TECHNICAL SPECIFICATIONS OF ITEMS

All equipment must be new; refurbished equipment will not be accepted.
All equipment must comply with the minimum requirements specified.
Images of the proposed equipment must be attached to the RFP submission.


	CBP- Camdex
(End User)

	Line Item
	Model #
	Product
	Description (Minimum Specifications)
	Qty
	Unit

	
	
	Soldering Station
	
	
	

	1
	9040
	Grounding Cord 
	Grounding Cord, Economy Coil
10 ft Over-All Length 
4mm Snap Size for connection to wrist strap or mat 
Desco 09040 or equal

	2
	Ea.

	2
	
	JTAG Box for eMMC data extraction 
	JTAG Box for eMMC data extraction 
Includes: 
-EasyJTAG Plus High Speed Interface Box
 -Z3X PreActivated Card with JTAG Activation 
-ISP1 1Bit Adapter PCB
 -ISP4 4Bit Adapter PCB
 -JTAG Adapter PCB 
Brand Name Only
 In-Country Warranty
	2
	Kit

	
	
	Photo Equipment
	
	
	

	3
	U3225QE
	31.5" Monitor 
	
31.5" monitor 
Features: 
Flat Screen Monitor 
4K UHD (3840 x 2160) Resolution
 IPS Black Panel Type
 Height-adjustable stand 
Integrated USB Hub
 Dell UltraSharp 32 4K Thunderbolt Hub Monitor - U3225QE or equal 
In-Country Warranty
	1
	Ea.

	4
	GVM1500D2
	LED Light Panel 
	RGB LED Light Panel (2-Light Kit)
 Features: 
2 75W LED panels
 2 diffusers 
2 Barndoors 
2 Light stands 
2 Power Adapters 
2 Power Cables 
1 Carry bag 
GVM 1500D or equal 
In-Country Warranty
	1
	Kit

	5
	SDCFE-512G-GN4NN 
	 512 GB Type B Memory Card
	Type B Memory Card
 512 GB
 SanDisk 512GB Extreme PRO CFexpress Type B Memory Card or equal 
	1
	Ea.

	6
	Nikon Z6 III
	Mirrorless Camera with lens
	Mirrorless Camera with 24-120mm f/4 Lens and Essentials+ Kit
 Full-frame mirrorless body and 24-120mm f/4  lens with a protective camera bag, a memory card, and memory card reader.
 Nikon Z6 III Mirrorless Camera with NIKKOR Z 24-120mm f/4  Lens and Essentials+ Kit or equal 
In-Country Warranty if applicable
	1
	Kit

	7
	NICCSWP2UV 
	Camera Control Software 
	Camera Control Software 
 Features:
 Remote camera control
 Live View
 Image Transfer 
Interval Timer Shooting 
Batch Processing 
Integration 
Must be compatible with CLIN 7
 Nikon Camera Control Pro 2.0 Software or equal 

	1
	Ea.

	8
	UL2873
	Desktop Microphone/Overhead Stand 
	Desktop Microphone/Overhead Stand
Adjustable desktop boom arm stand for microphones, cameras, and lights 
Features:
 3-Section Boom Arm 
Supports up to 3.3lb
 27.2" Max Height/Reach 
Ulanzi VIJIM LS25 or equal 
In-Country Warranty if applicable
	1
	Ea.

	9
	Anker 551 
	USB A to USB C Cable, Charger Cord 
	USB A to USB C Cable, Charger Cord (2 Pack, 10FT)
 For iPhone 17 Series, Samsung Galaxy Note 10/S10+ S10, LG V30
 Anker USB A to USB C Cable or equal  
	2
	Ea.

	10
	
	Plasticine Modeling Clay
	Reusable and Non-Drying Oil-Based Plasticine Modeling Clay, Color: Cream
	1
	Ea.

	11
	
PPS600
	Fractional Bureau Scale
	Fractional Bureau Scale 
L-shaped 
Reversible 
300 x 150mm
	1
	Ea.

	12
	
	Brown Butcher Paper Roll
	24" x 175' (2100")  Butcher Paper Roll 
Color: Brown
	2
	Ea.

	
	
	Data Server
	
	
	

	13
	C6ASPAT10AQ
	Ethernet Cable
	Ethernet Cable 
10ft  
Category 6 Augmented
 10 Gigabit Shielded Snagless
 Bandwidth up to 500MHz
 Connector Type: RJ45
 Up to 100W Power over Ethernet (PoE) Patch Cord 
10GbE STP Network Cable with Strain Relief 
Aqua Fluke Tested/Wiring is UL Certified/TIA
 In-Country Warranty
	4
	Ea.

	14
	UBUSWFLEXXG 
	4-port 10g Managed Network Switch
	Managed Network Switch
 4 x 10G Ethernet Ports 
82 Gb/s Switching Capacity 
Desktop and Wall mountable 
Includes Power Adapter 
1 x Gigabit Ethernet PoE-In Uplink Port 
61.01 Mpps forwarding rate
 Ubiquiti Networks UniFi Switch Flex XG 4-Port 10G Managed Network Switch or equal 
In-Country Warranty
	1
	Ea.

	15
	SNV3410-400G
	M.2 NVMe Solid State Drive (SSD)
	M.2 NVMe Internal Solid State Drive (SSD)
 Form Factor" M.2 2280 (22mm x 80mm)
 Usuable Capacity: 400GB
 Interface: PCI-Express 3.0 x4 
Synology SNV3410-400G or equal
 In-Country Warranty 
	2
	Ea.

	16
	E10G18-T1
	PCIe Expansion Card
	10GbE PCIe Expansion Card
 For Select Synology NAS Servers
 Supports 802.3an 10 Gb/s Ethernet
 Supports 802.3bz 2.5 & 5 Gb/s Ethernet
 Supports 802.3ab Gigabit Ethernet
 Supports 802.3u Fast Ethernet
 Supports 802.3x Flow Control
 PCIe 3.0 x4 Interface
 Full Duplex Network Operation Mode
 Auto Bandwidth Negotiation
 Synology E10G18-T1 10GbE PCIe Expansion Card or equal 
In-Country Warranty
	1
	Ea.

	17
	D4ES01-16G
	SO-DIMM Memory Module
	SO-DIMM (Small Outline Dual In-line Memory Module) 
Capacity: 16GB
 Type: DDR4
 Speed: 2666 MHz (PC4-21300) 
Error-Correcting Code (ECC) functionality 
D4ES01-16G or equal 
In-Country Warranty
 Synology 16GB DDR4 2666 MHz ECC SO-DIMM Memory Module or equal 
	2
	Ea.

	18
	ST16000NM000J
	Hard Disk Drive
	Hard Disk Drive
 Features:
 Storage Capacity: 16Tb
 Rotational Speed: 7200 rpm
 Interface: Sata 6gb/s
 Buffer: 256Mb
 512e Sector Size (bytes Per Sector): 512 
SEAGATE ST16000NM000 Hard Drive or equal 
	8
	Ea.

	19
	DS1621
	DiskStation + 6-Bay NAS Enclosure
	Diskstation 
Features: 
6 x 3.5"/2.5" SATA HDD/SSD Drive Bays
 2.2 GHz AMD Ryzen V1500B Quad-Core
 4GB of DDR4 ECC RAM
 4 x Gigabit Ethernet Ports
 3 x USB 3.2 Gen 1 Type-A | 2 x eSATA
 RAID 0, 1, 5, 6, 10, Hybrid, and JBOD
 Sequential Writes up to 2300 MB/s
 AES-NI Hardware Encryption Engine
 M.2 2280 SSD & 10GbE Expansion Slots
 In-Country Warranty
 
Synology DiskStation DS1621+ 6-Bay NAS Enclosure or equal 
In-Country Warranty
	1
	Ea.

	
	
	Forensic Workstations
	
	
	

	20
	CP2K32G56C46U5
	Desktop Memory Model 
	
	4
	Ea.

	21
	ST12000VN0008
	NAS Hard Drive 
	NAS Hard Drive 
Storage Capacity: 12TB
 Form Factor: 3.5" 
Interface: SATA III 6.0 Gb/s 
Rotational Speed: 7200 RPM
 Cache: 256MB
 Recording Technology: CMR (Conventional Magnetic Recording)
 Seagate Ironwolf ST12000VN0008 or equal  
	3
	Ea.

	22
	MZ-V9P4T0B/AM
	Internal Solid Hard Drive 
	Internal Solid State Hard Drive
 Capacity: 4TB
 Form Factor: M.2 2280
 Interface: PCIe Gen 4.0x4, NVMe 2.0
 Sequential Read Speed: Up to 7,450 MB/s for 
Sequential Write Speed: Up to 6,900 MB/s
 SAMSUNG 990 PRO SSD 4TB PCIe 4.0 M.2 2280 or equal 
In-Country Warranty
	2
	Ea.

	23
	TX401
	10G Ethernet PCIe Adapter
	10 Gigabit Ethernet PCIe Adapter
 PCIe 3.0 x4 Host Interface 
Includes:
 Full and Low-Profile Brackets 
Cat 6a Ethernet Cable 
1 x 10G Ethernet LAN Port 
Supports Windows 11/10/8.1/8/7, Servers 
TP-Link TX401 10G Ethernet PCIe Adapter or equal 
In-Country Warranty
	2
	Ea.

	24
	S2725QS
	Monitor 27"  
	27-inch 4K monitor with up to 120Hz refresh rate and dual 5W speakers
 Dell 27 Plus 4K Monitor or equal 
In-Country Warranty
	12
	Ea.

	25
	FCT2250
	Desktop
	Intel® Core™ Ultra 9 285 (24 cores, up to 5.6 GHz, 65 W)
 Includes:
 operating system Windows 11 Pro
 videocard NVIDIA® RTX™ 2000 ADA, 16 GB GDDR6, 4 mDP to DP adapters
 memory 32GB: 2 x 16 GB, DDR5, 5600 MT/s, non-ECC
 hard drive 1 TB, M.2 2280, TLC PCIe Gen4, SSD, SED Ready
 Dell Pro Max Tower T2 Desktop or equal 
In-Country Warranty
 
	4
	Ea.

	26
	6AX210
	Magnet Axiom
	Magnet Axiom Advanced 
1 year of software license 
Brand Name Only 
	1
	Ea.

	27
	B-CNR-05-001
	Inseyets Online Pro 
	Cellebrite UFED - Universal Forensics Extraction Device
 Inseyets Online Pro Software 
	1
	Ea.

	28
	S-AIS-20-001
	Inseyets Online Limited Unlocks Subscription
	Inseyets Online Limited Unlocks Subscription
 15 unlocks for mobile forensics
	15
	Ea.

	29
	
	GreyKey Software Suite
	
	1
	Ea.

	30
	
	MSAB XRY Pro Suite
	MSAB XRY Pro Suite
	1
	Ea.

	FBI- TEDAC 1: (Fixed)
(End User)

	Line Item
	Model #
	Product
	Description (Minimum Specifications)
	Qty
	Unit

	1
	FTK
	Two-Year Forensic Virtual License
	Forensic tool: digital forensics software for full-disk image collection processing and review. License Only 
Description: full-disk forensic images and process a wide range of data types from many sources, including Windows and Linux hard drives, CD’s and DVDs, thumb drives or other USB devices, network data and Internet storage, all in a centralized, secure database
 FTK Virtual License 
Brand Name Only
	1
	Ea.

	2
	B-UFD-10-001
	UFED - Universal Forensics Extraction Device. Two-Year UFED 4PC License Software
	Cellebrite UFED - Universal Forensics Extraction Device, latest version. UFED 4PC license Software for two years 
Forensic tool: digital forensics software for full-disk image collection processing and review
 Description: full-disk forensic images and process a wide range of data types from many sources, including Windows and Linux
 Brand Name Only
 
	1
	Ea.

	3
	B-UFD-10-013
	Cellebrite Physical Analyzer Two-Year Subscription
	Cellebrite Physical Analyzer, latest version. Stand Alone Subscription for two years 
Brand Name Only
	1
	Ea.

	4
	
	Two-Year Mobile Forensics and Data Recovery Software
	Mobile Forensics and Data Recovery Software for Two Years 
MSAB XRY EXTRACT and XAMN 
Brand Name Only
	1
	Ea.

	5
	
	Two-Year Disero License / V2 Forensics
	Software license for two years 
Description: Access, extract, decrypt and/or decode information out of unmanned aerial systems
 Disero License V2 Forensics 
Brand Name Only
	1
	Ea.

	6
	
	Two-Year CFID License
	CFID license (Hardware and Software) 
Software for CFID v 3.0 equipment for two years
 Brand Name Only
 In-Country Warranty
	1
	Ea.

	7
	TD4
	Forensic Duplicator 
	Drive Duplicator supporting SATA/SAS, USB, IDE, FireWire, m.2/NVMe forensic imaging through three write-blocked source ports:  SATA/SAS, PCIe, and USB 3.2 (Type-C) to Five destination ports:  SATA (x2), PCIe, and USB 3.2 (Type-C, x2)
 TD4.KIT+ADAPTERS 
Features:
 Multiple destination drive imaging
 PCIe drive hot swap
 Partition/file-system awareness
 Native support for PCIe, SAS and USB-C connections
 Color LCD touchscreen
 Audible feedback
 Simultaneous hashing
 Native image collection
 IT mode(bypass hash calculations)
Compatible with all existing Tableau Forensic drive adapters.
 Tableau TD4 Forensic Duplicator 
Brand Name Only
 In-Country Warranty if applicable
	2
	Set

	8
	IP-VRTBL-10
	VR Table
	VR-TABLE FOR EMMC, JTAG, FBUS 
Precision Probs
 Precision tool for non-invasive ISP reading and writing via EMMC, JTAG- without soldering 
10 arm (9 Vrarms + 1VR holder arm)
 Brand Name Only
 In-Country Warranty
 
	4
	Ea.

	9
	Z3X
	JTAG Box for eMMC data extraction 
	JTAG Box for eMMC data extraction 
Includes: 
- EasyJTAG Plus High Speed Interface Box.
 - Z3X PreActivated Card with JTAG Activation.
 - ISP1 1Bit Adapter PCB.
 - ISP4 4Bit Adapter PCB.
 - JTAG Adapter PCB.
 - E-Socket Adapter PCB.
 - USB2.0 Cable.
 Brand Name Only
 In-Country Warranty
 
	4
	Ea.

	10
	E36313A
	Triple Output Power Supply
	Bench Power Supply, DC, Programmable, 3 Output
 160W Triple Output Power Supply, 6V, 10A & 2X 25V, 2A
 Output Rating- 160 W
 Output 1: 0 to 6 V, 0 to 10 A
 Output 2: 0 to 25 V, 0 to 2 A
 Output 3: 0 to 25 V, 0 to 2 A
 Programming Accuracy ±(% of output + offset)
 Voltage: 0.03% + 3 mV, 0.03% + 5 mV, 0.03% + 5 mV
 Current: 0.05% + 4 mA, 0.04% + 3 mA, 0.04% + 3 mA
 Ripple & Noise (20 Hz to 20 MHz)
 Normal Mode Voltage: <350 µVrms/ 2 mV p-p, < 1 mVrms/ 5 mVpp, < 1 mVrms/ 5 mVpp
 Normal-mode current: <4 mA rms, <2 mA rms, <1 mA rms
 Readback Accuracy ±(% of output + offset)
 Voltage: 0.04% + 3 mV, 0.03% + 5 mV, 0.03% + 5 mV
 Current: + 0.05% + 5 mA, 0.04% + 3 mA, 0.04% + 3 mA
 Low Range Current, 20 mA: 0.25% + 80 uA
 E36313A Keysight or equal 
In-Country Warranty
	4
	Ea.

	11
	REVELPROG-IS
	Programmer Memory
	Programmer memory for flash memory FRAM
 REVELPROG-IS 
Brand Name Only
	2
	Ea.

	12
	Precision 7960 
	Workstation
	Processor: Intel® Xeon® W7-3465X, 28 cores
 Precision 7960 Tower Workstation 
Operating system: Red Hat Linux® 9.3 Enterprise WS
 Graphics Card: NVIDIA® RTX™ A400
 Memory: 128 GB DDR5
 Storage: 1 TB Performance SSD, SED Ready
 Dell Precision 7960 Tower Workstation or equal 
In-Country Warranty
	4
	Ea.

	13
	Pro Max 18 
	Laptop
	Laptop
 Processor: Intel® Core™ Ultra 7 265HX vPro®, 20 cores
 Operating system: Windows 11 Pro
 Graphics Card: NVIDIA® RTX™ PRO 1000 Blackwell Generation
 Memory: 32 GB DDR5
 Storage: 512 GB Performance SSD, SED Ready
 Display: 18" Non-Touch QHD+
 Dell Pro Max 18 Plus Laptop or equal 
In-Country Warranty
	4
	Ea.

	14
	NID78024120
	Digital Camera
	Digital Camera - 
Features: 
24.5MP FX-Format BSI CMOS Sensor
 EXPEED 6 Image Processing Engine
 UHD 4K30 Video; N-Log & 10-Bit HDMI Out
 Multi-CAM 3500 II 51-Point AF System
 273-Point Hybrid AF with Eye Detection
 3.2" 2.36m-Dot Tilting Touchscreen LCD
 7 fps Shooting, 12 fps in Live View
 Extended ISO 50-204800
 Built-In Wi-Fi and Bluetooth
 AF-S NIKKOR 24-120mm f/4G ED VR Lens
 DSLR Camera Nikkon D780 with 24-120mm Lens or equal 
In-Country Warranty if applicable 
	1
	Ea

	FBI- TEDAC 2 Simplified Kit (Mobile)
(End User)

	Line Item
	Model #
	Product
	Description (Minimum Specifications)
	Qty
	Unit

	1
	FTK
	Two-Year Forensic Virtual LicenseToolkit
	Forensic tool: digital forensics software for full-disk image collection processing and review. Two (2) years License and warranty Only.
 Description: full-disk forensic images and process a wide range of data types from many sources, including Windows and Linux hard drives, CD’s and DVDs, thumb drives or other USB devices, network data and Internet storage, all in a centralized, secure database
 FTK Virtual License 
Brand Name Only
	1
	Ea.

	2
	
	Disero License, V2 Forensics
	Software license for two years 
Description: Access, ectract, decrypt and/or decode information out of unmaned aerial systems
 Disero License V2 Forensics 
Brand Name Only
	1
	Ea.

	3
	
	Two-Year CFID License
	CFID license (Hardware and Software) 
Software for CFID v 3.0 equipment for two years
 Brand Name Only
 In-Country Warranty
	1
	Ea. 

	4
	TD4
	Forensic Duplicator 
	Drive Duplicator supporting SATA/SAS, USB, IDE, FireWire, m.2/NVMe forensic imaging through three write-blocked source ports:  SATA/SAS, PCIe, and USB 3.2 (Type-C) to Five destination ports:  SATA (x2), PCIe, and USB 3.2 (Type-C, x2)
 TD4.KIT+ADAPTERS 
Features:
 Multiple destination drive imaging
 PCIe drive hot swap
 Partition/file-system awareness
 Native support for PCIe, SAS and USB-C connections
 Color LCD touchscreen
 Audible feedback
 Simultaneous hashing
 Native image collection
 IT mode(bypass hash calculations)
* Compatible with all existing Tableau Forensic drive adapters.
 Tableau TD4 Forensic Duplicator  
Brand Name Only
 In-Country Warranty if applicable
 
	1
	Set

	5
	IP-VRTBL-10
	VR Table
	VR-TABLE FOR EMMC, JTAG, FBUS 
Precision Probs
 Precision tool for non-invasive ISP reading and writing via EMMC, JTAG- without soldering 
10 arm (9 Vrarms + 1VR holder arm)
 Brand Name Only 
In-Country Warranty
 
	1
	Ea. 

	6
	Z3X
	JTAG Box for eMMC data extraction 
	JTAG Box for eMMC data extraction 
Includes: 
- EasyJTAG Plus High Speed Interface Box.
 - Z3X PreActivated Card with JTAG Activation.
 - ISP1 1Bit Adapter PCB.
 - ISP4 4Bit Adapter PCB.
 - JTAG Adapter PCB.
 - E-Socket Adapter PCB.
 - USB2.0 Cable.
 Brand Name Only 
In-Country Warranty
	1
	Set

	7
	E36313A
	Triple Output Power Supply
	Bench Power Supply DC, Programmable, 3 Output 160W Triple Output Power 
E36313A Keysight or equal 
In-Country Warranty
	1
	Ea. 

	8
	REVELPROG-IS
	Programmer Memory
	Programmer memory for flash memory FRAM
 REVELPROG-IS 
Brand Name Only
 In-Country Warranty if applicable
	1
	Ea. 

	9
	Pro Max 18 
	Laptop
	Laptop
 Processor: Intel® Core™ Ultra 7 265HX vPro®, 20 cores
 Operating system: Windows 11 Pro
 Graphics Card: NVIDIA® RTX™ PRO 1000 Blackwell Generation
 Memory: 32 GB DDR5
 Storage: 512 GB Performance SSD, SED Ready
 Display: 18" Non-Touch QHD+
 Dell Pro Max 18 Plus Laptop or equal 
In-Country Warranty
	1
	Ea.





1
SENSITIVE BUT UNCLASSIFIED

